For 1990-2009 cars

### Removal Procedure

1. Open the doors
2. Partially remove the auxiliary weatherstrip (2).
3. Gently pry the reveal molding (1) from the top working towards the air inlet panel.
4. Release the reveal molding from the pinchweld flange.
5. Remove the reveal molding from the windshield pillar.

### Installation Procedure

1. Install the reveal molding under the air inlet panel grille.
2. Align the reveal molding to the pinchweld flange and to the top roof header.
3. Press the reveal molding (1) onto the pinchweld flange.
4. Reposition the auxiliary weatherstrip (2).
5. Close the doors.