For 1990-2009 cars

### Removal Procedure

1. Open the rear door.
2. Remove the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
3. Remove the rear door opening weatherstrip (2) from the door opening pinchweld flange (1).
4. Remove the rear door opening weatherstrip from the vehicle.

### Installation Procedure

1. Position the rear door opening weatherstrip to the pinchweld flange.
2. Starting at the upper rear corner, press the rear door opening weatherstrip (2) onto the pinchweld flange (1) until it is fully seated.
3. Install the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
4. Pull the cord (3) on the rear door opening weatherstrip ensuring the weatherstrip lip overlaps the interior trim panels and headliner.
5. Close the rear door.