For 1990-2009 cars

#### Tools Required

J 44225 Balance Shaft Bearing Remover/Installer

1. Position the cylinder block so the cylinder head deck face is down and identify the following:

• | The left balance shaft bearings are in the shorter length balance shaft journal (3) and (4).

• | The right balance shaft - outer diameter is grooved, bearings are in the longer length balance shaft journal (1) and (2).

2. Identify the following:

• | Bearings (2) and (3) are the front bearings and bearings (1) and (4) are the rear bearings.

• | The rear bearings (1) and (4) have a slightly larger diameter than the front bearings (2) and (3). This allows for easier removal and installation of the front bearings. The rear bearings also have notches on them.

Important: It may help to stand the block on end to aid in positioning the swivel end of J 44225 .

3. Install J 44225 into the right balance shaft bearing bore.
4. Position the swivel end inside lip of J 44225 against the frontside of the rear bearing.
5. Turn the nut clockwise to remove the bearing.
6. Remove and discard the right rear bearing (1).
7. Install J 44225 into the right balance shaft bearing bore.
8. Position the swivel end inside lip of J 44225 against the frontside of the front bearing.
9. Turn the nut clockwise to remove the bearing.
10. Remove and discard the right front bearing (1).
11. Install J 44225 into the left balance shaft bearing bore.
12. Position the swivel end inside lip of J 44225 against the frontside of the rear bearing.
13. Turn the nut clockwise to remove the bearing.
14. Remove and discard the left rear bearing (1).
15. Install J 44225 into the left balance shaft bearing bore.
16. Position the swivel end inside lip of J 44225 against the frontside of the front bearing.
17. Turn the nut clockwise to remove the bearing.
18. Remove and discard the left front bearing (1).