For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
3. Remove the push-pins from the inner wheelhouse liner.
4. Remove the inner wheelhouse liner from the vehicle.
5. Remove the push-pins from the outer wheelhouse liner.
6. Remove the outer wheelhouse liner (2).

### Installation Procedure

1. Install the outer wheelhouse liner (2) to the vehicle.
2. Install the rearward push-pin into the outer wheelhouse liner.
3. Install the remaining push-pins into the outer wheelhouse liner.
4. Install the inner wheelhouse liner to the vehicle.
5. Install the push-pins into the inner wheelhouse liner.
6. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
7. Lower the vehicle.