For 1990-2009 cars

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement.
2. Remove the bolt (3) securing the A/C compressor hose/pipe bracket (2) to the engine lift bracket (1).
3. Carefully disengage the engine wiring harness conduit (4) from the engine lift bracket (1).
4. Remove the 3 generator bolts.
5. Remove the bolts securing engine lift bracket to the engine.
6. Remove the engine lift bracket from the engine.

### Installation Procedure

1. Position the engine lift bracket to the engine.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolts securing engine lift bracket to the engine.

• | Tighten the bolts in sequence to 5 N·m (44 lb in).

• | Tighten the bolts in sequence to 50 N·m (37 lb ft).

3. Position the generator to the engine.
4. Install the generator bolts and tighten in sequence to 50 N·m (37 lb ft).
5. Engage the engine wiring harness conduit (4) to the engine lift bracket (1).
6. Install the bolt (3) securing the A/C compressor hose/pipe bracket (2) to the engine lift bracket (1).

Tighten the bolt to 9 N·m (80 lb in).

7. Install the drive belt. Refer to Drive Belt Replacement.