For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear bumper impact bar. Refer to Rear Bumper Impact Bar Replacement.

1 | Rear Bumper Impact Bar Reinforcement Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 160 N·m (118 lb ft)
2 | Rear Bumper Impact Bar Reinforcement Bolt (Qty: 4) Tighten 100 N·m (74 lb ft)
3 | Rear Bumper Impact Bar Reinforcement

#### Procedure

1. Disconnect any electrical connectors.
2. Transfer components as necessary.