For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner outlet duct. Refer to Air Cleaner Resonator Outlet Duct Replacement.
2. Release the air cleaner upper housing retainer clips (1).
3. Open the air cleaner upper housing (1).
4. Remove the air filter element (2) from the lower air cleaner housing.
5. Inspect the air cleaner assembly for debris or damage and repair as necessary.

### Installation Procedure

1. Install the air filter element (2) to the lower air cleaner housing.
2. Close the air cleaner upper housing (1).
3. Latch the air cleaner upper housing retainer clips (1).
4. Install the air cleaner outlet duct. Refer to Air Cleaner Resonator Outlet Duct Replacement.