For 1990-2009 cars

### Removal Procedure

1. Disconnect the engine wiring harness electrical connector (4) from the exhaust camshaft position (CMP) sensor (5).
2. Remove the exhaust CMP sensor retaining bolt.
3. Remove the exhaust CMP sensor from the cylinder head.

### Installation Procedure

1. Lightly lubricate the O-ring seal with clean engine oil.
2. Install the exhaust CMP sensor into the cylinder head.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the exhaust CMP sensor bolt.

Tighten
Tighten the CMP sensor bolt to 10 N·m (89 lb in).

4. Connect the engine wiring harness electrical connector (4) to the exhaust CMP sensor (5).