For 1990-2009 cars

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement.
2. Remove the 2 clutch actuator cylinder bolts (3).
3. Remove the clutch actuator cylinder (1) from the input shaft bearing retainer (2).

### Installation Procedure

1. Position the clutch actuator cylinder (1) to the input shaft bearing retainer (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 2 clutch actuator cylinder bolts (3).

Tighten
Tighten the clutch actuator cylinder bolts to 8 N·m (71 lb in).

3. Install the transmission. Refer to Transmission Replacement.