For 1990-2009 cars

### Removal Procedure

1. Remove the grille. Refer to Grille Replacement .
2. Disconnect the horn assembly electrical connector.
3. Remove the bolt that retains the horn assembly to the radiator support.
4. Remove the horn assembly from the body.

### Installation Procedure

1. Install the horn assembly to the radiator support.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolt that retains the horn assembly to the radiator support.

Tighten
Tighten the bolt to 10 N·m (88 lb in).

3. Connect the horn assembly electrical connector.
4. Install the grille. Refer to Grille Replacement .