For 1990-2009 cars

## Compressor Clutch Plate/Hub Assembly Replacement LH8

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the compressor. Refer to Air Conditioning Compressor Replacement

1 | Clutch Plate Retaining Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 18 N·m (13 lb ft)
2 | A/C Washer Refer to Sealing Washer Replacement.
3 | Clutch Plate Assembly
4 | Clutch Hub/Bearing Snap Ring
5 | Clutch Hub/Bearing Assembly

## Compressor Clutch Plate/Hub Assembly Replacement LLV, LLR

### Removal Procedure

1. Remove the compressor. Refer to Air Conditioning Compressor Replacement.
2. Remove the clutch plate retaining bolt (1).
3. Remove the clutch plate assembly (2).
4. Remove the clutch hub/bearing snap ring (3).
5. Remove the clutch hub/bearing assembly (4).

### Installation Procedure

1. Install the clutch hub/bearing assembly (4).
2. Install the clutch hub/bearing snap ring (3).
3. Install the clutch plate assembly (2).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the clutch plate retaining bolt (1). Tighten the bolt to 18 N·m (13 lb ft).
5. Install the compressor. Refer to Air Conditioning Compressor Replacement.