For 1990-2009 cars

#### Tools Required

J 39400-A Halogen Leak Detector

### Removal Procedure

1. Recover the refrigerant from the system. Refer to Refrigerant Recovery and Recharging .
2. Remove the generator. Refer to Generator Replacement .
3. Remove the drive belt. Refer to Drive Belt Replacement for the 2.9L engine or Drive Belt Replacement for the 3.7L engine.
4. Disconnect the compressor electrical connectors.

Important: Some system pressure may still exist in the A/C compressor crankcase after you evacuate the system.

5. Remove the discharge hose bolt from the compressor.
6. Remove the suction hose from the compressor.
7. Remove the compressor hose assembly blocks from the compressor.
8. Remove the compressor mounting bolts from the compressor (1).
9. Remove the compressor .
10. Drain and measure the compressor oil. Refer to Air Conditioning Compressor Oil Balancing .

### Installation Procedure

1. Adjust the proper amount of oil to the replacement compressor. Refer to Refrigerant System Capacities .
2. Install the compressor.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the compressor mounting bolts to the compressor (1).

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

4. Install the compressor hose assembly blocks to the compressor.
5. Install the suction hose to the compressor
6. Install the discharge hose bolt to the compressor (1).

Tighten
Tighten the bolts to 33 N·m (24 lb ft).

7. Connect the compressor electrical connectors.
8. Install the drive belt. Refer to Drive Belt Replacement for the 2.9L engine or Drive Belt Replacement for the 3.7L engine.
9. Install the generator. Refer to Generator Replacement .
10. Evacuate and recharge the A/C system. Refer to Refrigerant Recovery and Recharging .
11. Leak test the fittings of the components using the J 39400-A .