For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the sunshade to the full open position.
2. Remove the sunroof front trim cover. Refer to Sunroof Front Trim Cover Replacement.
3. Remove the sunroof motor. Refer to Power Sunroof Motor Replacement.

1 | Sunroof Cam Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
2 | Sunroof Cam Plate
3 | Sunroof Cam Tip Ensure that the chamfered edge of the gear is directed upward.