For 1990-2009 cars

### Removal Procedure

1. Remove the spark plug wire from the spark plug.

• | Twist each spark plug 1/2 turn.

• | Pull only on the boot in order to remove the wire from each spark plug.

2. Remove the spark plug wire from the ignition coil.

• | Twist each spark plug boot 1/2 turn.

• | Pull only on the boot in order to remove the wires from the ignition coil.

### Installation Procedure

1. Install the spark plug wire to the ignition coil.
2. Install the spark plug wire to the spark plug.
3. Inspect the wires for proper installation:

• | Push sideways on each boot in order to inspect the seating.

• | Reinstall any loose boot.