For 1990-2009 cars

### Removal Procedure

1. Remove the rear side access door trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the bolt retaining the rear side access door check link to the body.
3. Remove the nuts retaining the rear side access door check link to the door.
4. Remove the rear side access door check link (1) from the door.

### Installation Procedure

1. Install the rear side door check link to the door, ensuring the alignment mark (1) faces upward.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the nuts retaining the rear side door check link to the door and tighten to 9 N·m (80 lb in).
3. Install the bolt retaining the rear side access check link to the body and tighten to 25 N·m (18.4 lb ft).
4. Install the rear side access door trim panel. Refer to Rear Side Door Trim Panel Replacement.