For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Conditioning Compressor Bolt | 50 N·m | 37 lb ft
Battery Cable to Battery Nut | 9 N·m | 80 lb in
Battery Retainer Nut | 15 N·m | 11 lb ft
Generator Mounting Bolt | 50 N·m | 37 lb ft
Generator Output BAT Terminal Nut | 20 N·m | 15 lb ft
Generator Positive Cable to Underhood Fuse Block Nut | 10 N·m | 89 lb in
Negative Battery Cable to Battery Tray Bolt | 9 N·m | 80 lb in
Negative Battery Cable to Engine Block Bolt | 35 N·m | 26 lb ft
Positive Battery Cable to Starter Terminal Nut | 9 N·m | 80 lb in
Positive Battery Cable to Underhood Fuse Block Nut | 10 N·m | 89 lb in
Starter Motor Bolt/Nut | 50 N·m | 37 lb ft
Starter Solenoid S Terminal Nut | 3.5 N·m | 31 lb in