For 1990-2009 cars

## Engine Flywheel Replacement with Automatic Transmission

#### Special Tools

J 45059 Angle Meter

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement.
2. Remove and discard the flywheel bolts.
3. Remove the flywheel.

### Installation Procedure

1. Position the flywheel to the crankshaft

Caution: Refer to Fastener Caution in the Preface section.

2. Install the new flywheel bolts and tighten to 40 N·m (30 lb ft) plus an additional 45 degrees using the J 45059 .
3. Install the transmission. Refer to Transmission Replacement.

## Engine Flywheel Replacement with Manual Transmission

#### Special Tools

J 45059 Angle Meter

### Removal Procedure

1. Remove the clutch assembly. Refer to Clutch Assembly Replacement.
2. Remove and discard the flywheel bolts.
3. Remove the flywheel.

### Installation Procedure

1. Position the flywheel to the crankshaft

Caution: Refer to Fastener Caution in the Preface section.

2. Install the new flywheel bolts and tighten to 40 N·m (30 lb ft) plus an additional 45 degrees using the J 45059 .
3. Install the clutch assembly. Refer to Clutch Assembly Replacement.