For 1990-2009 cars

### Removal Procedure

Warning: Refer to Halogen Bulb Warning in the Preface section.

Caution: Avoid touching the bulb or letting the bulb come in contact with anything damp. Oil from your skin or moisture on the bulb can cause the bulb to explode when the bulb is turned on. If either comes in contact with the bulb, clean the bulb with alcohol or a suitable degreaser and wipe the bulb dry.

1. Ensure that the headlamp switch is in the OFF position.
2. Ensure that the ignition switch is in the LOCK position.
3. Open the hood.
4. Release the locking tab (1) on the park, turn, daytime running lamp assembly by using a flat-bladed tool and pushing the tab on the lamp outward toward the fender.
5. Rotate the outward edge of the lamp assembly forward.
6. Release the park/turn signal lamp socket (2) by rotating the socket a quarter turn counter-clockwise.
7. Remove the park, turn signal lamp bulb (3).
8. Repeat steps 6 and 7 for the daytime running lamp socket (4) and bulb (5).

### Installation Procedure

1. Secure the bulbs (3,5) into the bulb sockets (2,4) and to the lamp assembly.
2. Insert the inside edge of the lamp tabs to the grille support.
3. Rotate the lamp assembly into the fender bracket.
4. Push on the outboard edge of the lamp until an audible click is heard, when the lamp assembly is secure to the fender.
5. Inspect the lamps for proper operation.