For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.
2. Remove the right air outlet assembly from the trim plate.
3. Remove the left air outlet assembly from the trim plate.

### Installation Procedure

1. Install the left air outlet assembly to the trim plate.
2. Install the right air outlet assembly to the trim plate.
3. Install the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.