For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjuster Plug - Allen Head

- First Pass

15 N·m

11 lb ft

- Final Pass

25 Degrees Back

Adjuster Plug - Hex Head

- First Pass

12 N·m

106 lb in

- Final Pass

105 Degrees Back

Adjuster Plug Lock Nut | 60 N·m | 44 lb ft
Cylinder Pipe Fittings Cylinder End | 15 N·m | 11 lb ft
Cylinder Pipe Fittings Valve End | 15 N·m | 11 lb ft
Flow Control Valve Fitting | 75 N·m | 55 lb ft
Inner Tie Rod End | 88 N·m | 65 lb ft
Lower Intermediate Shaft to Power Steering Gear Input Shaft Pinch Bolt | 45 N·m | 33 lb ft
Outer Tie Rod Jam Nut - 14 mm Tie Rod | 70 N·m | 52 lb ft
Outer Tie Rod Jam Nut - 16 mm Tie Rod | 75 N·m | 55 lb ft
Outer Tie Rod Retaining Nut

- First Pass

45 N·m

33 lb ft

- Final Pass

95 Degrees

Power Steering Gear isolator to the Frame Mounting Bolts | 100 N·m | 74 lb ft
Power Steering Gear to the Frame Mounting Bolts | 130 N·m | 96 lb ft
Power Steering Hose Assembly Clips to the Frame Mounting Bolts | 9 N·m | 79 lb in
Power Steering Hose Assembly to the Power Steering Gear Bolt | 12 N·m | 106 lb in
Power Steering Hose Assembly (Pressure Hose) to the Power Steering Pump | 25 N·m | 18 lb ft
Power Steering Hose Assembly to the Power Steering Gear Bolt | 12 N·m | 106 lb in
Power Steering Pump Bracket Mounting Bolts | 50 N·m | 37 lb ft
Power Steering Pump Mounting Bolts | 25 N·m | 18 lb ft