For 1990-2009 cars

#### Special Tools

J 45299 Engine Preluber

For equivalent regional tools, refer to Special Tools.

Caution: Refer to Fastener Caution in the Preface section.

Note: A constant/continuous flow of clean engine oil is required to properly prime the engine. Be sure to use an approved engine oil as specified in the owners manual.

1. Remove the engine oil filter, fill with clean engine oil, and reinstall. Tighten the oil filter to 30 N·m (22 lb ft).
2. Remove the engine block oil gallery plug (1).
3. Install the M16 x 1.5 adapter P/N 509375.
4. Install the flexible hose to the adapter and open the valve.
5. Pump the handle on J 45299 preluber to flow a minimum of 1-2 quarts of engine oil. Observe the flow of engine oil through the flexible hose and into the engine assembly.
6. Close the valve and remove the flexible hose and adapter from the engine.
7. Install the oil pressure sensor. Tighten the oil pressure sensor to 35 N·m (26 lb ft).
8. Top-off the engine oil to the proper level.