For 1990-2009 cars

Service the exhaust hangers individually in order to retain the support of the exhaust system.

### Removal Procedure

Warning: Refer to Exhaust Service Warning in the Preface section.

Warning: Refer to Protective Goggles and Glove Warning in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Note: Do not use oil base lubricants.

2. Apply a soapy solution to the following in order to ease the removal of the hanger (1):

• | The frame support bracket rod (2)

• | The exhaust pipe hanger rod (3)

3. Pry the exhaust pipe hanger (1) free from the following:

• | The frame support bracket rod (2)

• | The exhaust pipe hanger rod (3)

### Installation Procedure

Note: Do not use oil base lubricants.

1. Apply a soapy solution to the following in order to ease the installation of the hanger (1):

• | The frame support bracket rod (2)

• | The inner diameter of the exhaust pipe hanger (1)

• | The exhaust pipe hanger rod (3)

2. Press the exhaust pipe hanger (1) over the following:

• | The frame support bracket rod (2)

• | The exhaust pipe hanger rod (3)

3. Lower the vehicle.