For 1990-2009 cars

#### Tools Required

• | J-41816 Crankshaft Balancer Remover

• | J 41816-2 Crankshaft End Protector

• | J-41816-3 Crankshaft Balancer Remover Legs

1. Remove and discard the crankshaft balancer bolt.
2. Install J 41816-2 into the end of the crankshaft.

Important: Do not pull on outer edge of the crankshaft balancer.

Important: The friction washer may come off with the crankshaft balancer.

3. Use J-41816 and J-41816-3 to remove the crankshaft balancer.
4. Remove J 41816-2 .