For 1990-2009 cars

## Engine Coolant Fan Shroud Replacement LLV, LLR

### Removal Procedure

1. Remove the radiator hose-outlet. Refer to Radiator Outlet Hose Replacement .
2. Release the differential vent hose retainer.
3. Release the A/C suction hose retainer.
4. Release the A/C discharge hose retainer.
5. Rotate the slip ring counterclockwise from under the fan shroud.
6. Remove the fan shroud (3).

### Installation Procedure

1. Install the fan shroud (3) to the vehicle.
2. Rotate the slip ring to the original position.
3. Install the differential vent hose retainer.
4. Install the A/C suction hose retainer.
5. Install the A/C discharge hose retainer.
6. Install the radiator hose-outlet. Refer to Radiator Outlet Hose Replacement .