For 1990-2009 cars

1. Inspect the 1-2 accumulator piston (56) for the following conditions:

• | Porosity

• | Cracks

• | Scoring

• | Nicks and Scratches

2. Install a 1-2 accumulator piston oil seal ring (55) on the 1-2 accumulator piston (56).
3. Inspect the 1-2 accumulator housing for the following conditions:

• | Porosity

• | Cracks

• | Scoring

• | Nicks and Scratches

• | Debris or blocked passages

Important: Some models may not use an outer 1-2 accumulator spring (54).

4. Install the 1-2 inner (104) and outer (54) accumulator springs.
5. Install the 1-2 accumulator piston (56).