For 1990-2009 cars

### Removal Procedure

1. Remove the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.
2. Remove the 3 screws that retain the radio to the instrument panel (I/P).
3. Partially remove the radio disengaging the radio rear alignment locator to gain access to the electrical connectors.
4. Disconnect the radio antenna cable.
5. Disconnect the electrical connectors to the radio.
6. Remove the radio from the vehicle.

### Installation Procedure

1. Position the radio to the I/P.
2. Connect the electrical connectors to the radio.
3. Connect the radio antenna cable to the radio.
4. Position the radio rear alignment locator into the I/P substrate installing the radio to the I/P.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the 3 screws that retain the radio to the I/P.

Tighten
Tighten the screws to 2 N·m (18 lb in).

6. Install the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.
7. Program the replacement radio. Refer to Control Module References.