For 1990-2009 cars

### Removal Procedure

1. Grasp the lower center pillar trim panel and gently pull the panel away from the body to release the fasteners.
2. Remove any fasteners that may have pulled away from the panel and reinstall them to the back of the panel.
3. Slide the panel forward so the panel unhooks from around the front door frame.
4. Remove the lower center pillar trim panel from the vehicle.

### Installation Procedure

1. Position the lower center pillar trim panel so that the front edge hooks around the front door frame.
2. Ensure that the panel fasteners are aligned with the holes in the body.
3. Install the panel by pushing firmly against the body to seat the panel fasteners.