For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear bumper step pad. Refer to Rear Bumper Step Pad Replacement.
2. Remove the rear bumper step center pad. Refer to Rear Bumper Step Center Pad Replacement.

1 | Rear Bumper Impact Bar Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Rear Bumper Impact Bar Bracket (Qty: 8) Tighten 40 N·m (30 lb ft)
3 | Rear Bumper Impact Bar