For 1990-2009 cars

## Console Replacement Small W/ Manual Transmission

### Removal Procedure

1. Release the retaining strips on the shift lever boot.
2. Remove the inside rear seat track bolts on both front seats.
3. Lift up on the console to release the 4 retainers.
4. Remove the console from the vehicle.

### Installation Procedure

1. Position the console to the floor panel.
2. Ensure the retainers are indexed to the corresponding holes in the floor panel.
3. Push downward on the console seating the retainers.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the seat track bolts on both front seats.

Tighten
Tighten the bolts to 53 N·m (39 lb ft).

5. Attach the retaining strips on the shift lever bezel.