For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws securing the switch plate assembly to the door trim panel.
2. Lift the front of the switch plate up to disengage clip.
3. Remove the switch plate out of the door trim panel opening.
4. Disconnect the electrical connectors (3, 4) from the switches (2, 5).
5. Remove the switch plate assembly (1) from the vehicle.
6. If replacing only the switches, remove the switches from the plate.
7. If replacing only the switch plate, retain the switches for transfer.

### Installation Procedure

1. Install the switches (2, 5) to the switch plate (1).
2. Connect the electrical connectors (3, 4) to the switches (2, 5).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the switch plate assembly to the door trim panel with the 2 screws and tighten to 2 N·m (18 lb in).