For 1990-2009 cars

### Removal Procedure

1. Open the rear side access door.
2. Remove the bolts retaining the lower side access door striker to the body.
3. Remove the lower side access door striker from the body.

### Installation Procedure

1. Install the lower side access door striker to the body.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts retaining the lower side access door striker to the body.

Tighten
Tighten the lower side access door striker bolts to 25 N·m (18 lb ft).

3. Close the rear side access door.