For 1990-2009 cars

### Removal Procedure

1. Remove the electric motor actuator. Refer to Electric Motor Actuator Replacement .
2. Remove the left differential carrier assembly bushing and mounting bracket. Refer to Differential Carrier Assembly Bushing and Bracket Replacement .
3. Remove the disconnect housing bolts.
4. Remove the disconnect housing.
5. Remove the clutch fork, clutch assembly, thrust washer, and gasket from the disconnect housing.

### Installation Procedure

1. Install the clutch fork, clutch assembly, thrust washer, and gasket in the disconnect housing.
2. Install the disconnect housing.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the disconnect housing bolts.

Tighten
Tighten the disconnect housing retaining bolts to 60 N·m (44 lb ft).

4. Install the left differential carrier mounting bracket. Refer to Differential Carrier Assembly Bushing and Bracket Replacement .
5. Install the electric motor actuator. Refer to Electric Motor Actuator Replacement .