For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel cluster (IPC) bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement.
2. Remove the IPC. Refer to Instrument Cluster Replacement.
3. Remove the screws retaining the IPC lens.
4. Remove the lens from the IPC.

### Installation Procedure

1. Install the lens to the IPC.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the screws to the IPC lens.

Tighten
Tighten the screws to 1.5 N·m (14 lb in).

3. Install the IPC. Refer to Instrument Cluster Replacement.
4. Install the IPC bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement.