For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip Remover or Equivalent

### Removal Procedure

1. Open the rear door.
2. Remove the weatherstrip from around the door by inserting J 38778 , or equivalent, under the weatherstrip and releasing the integral retainers (2) from the door frame.
3. Remove the weatherstrip from the rear door.

### Installation Procedure

1. Position the weatherstrip to the rear door.
2. Install the weatherstrip around the rear door frame using the integral retainers (2).
3. Close the rear door.