For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws securing the switch plate assembly to the door trim panel.
2. Lift the switch plate up and out of the door trim panel.
3. Disconnect the electrical connectors from the switch module.
4. Remove the switch plate assembly from the vehicle.
5. If replacing only the switch module, remove the module from the switch plate.
6. If replacing only the switch plate, retain the switch module for transfer.

### Installation Procedure

1. Install the switch module to the switch plate.
2. Connect the electrical connector to the switch module.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the rear switch plate assembly to the door trim panel with the 2 screws and tighten to 2 N·m (18 lb in).