For 1990-2009 cars

### Removal Procedure

1. Open the sunshade to the full open position.
2. Remove the sunroof front trim cover. Refer to Sunroof Front Trim Cover Replacement.
3. Remove the sunroof motor. Refer to Power Sunroof Motor Replacement.

Note: Note the location of the bolts, size and color when removing, for proper installation.

4. Remove the screws from around the lower frame.
5. Remove the lower frame from sunroof module.

### Installation Procedure

1. Install the lower frame to the sunroof module.

Caution: Refer to Fastener Caution in the Preface section.

2. Tighten the screws to the lower frame of the sunroof module.

Install the bolts, size and color to the proper location.

Tighten
Tighten the screw to 3 N·m (27 lb in).

3. Push the sunroof window to the full open position. This will allow the window, motor and cables to be timed.
4. Install the sunroof motor. Refer to Power Sunroof Motor Replacement.
5. Install the sunroof front trim cover. Refer to Sunroof Front Trim Cover Replacement.
6. Verify operations of the sunroof window.