For 1990-2009 cars

#### Tools Required

J 29714-A Servo Cover Depressor

1. Install the J 29714-A .

Important: If cover does not move inwards with tool, use a block of wood or suitable material and lightly tap on cover using a hammer to free up cover in bore.

2. Tighten the J 29714-A bolt to compress the servo cover.
3. Remove the servo cover retaining ring (29) and the J 29714-A .
4. Remove the servo cover (28) and O-ring seal (27). If the servo cover seems to be hung up on the seal, cut and remove the O-ring seal before removing the cover.
5. Remove the 2-4 servo assembly.