For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank module. Refer to Fuel Tank Module Replacement .
2. Disconnect the fuel level sensor electrical connector from the module cover.
3. Disengage the locking tab (1) on the module bucket.
4. Slide the fuel level sensor downward off from the module bucket.

### Installation Procedure

1. Align the edges of the fuel level sensor with the slots in the module bucket.
2. Slide the fuel level sensor into position, ensure the locking tab (1) is fully engaged.
3. Connect the fuel level sensor electrical connector to the module cover.
4. Install the fuel tank module. Refer to Fuel Tank Module Replacement .