For 1990-2009 cars

1. Inspect the 3-4 accumulator piston (44) for the following conditions:

• | Porosity

• | Cracks

• | Scoring

• | Nicks and scratches

2. Install the 3-4 accumulator piston oil seal ring (45) on the 3-4 accumulator piston (44).
3. Install the 3-4 accumulator piston (44) and seal assembly into the bore.
4. Inspect the 3-4 accumulator spring (46) for cracks.

Note: Some models do not use a 3-4 accumulator spring.

5. Install the 3-4 accumulator spring.