For 1990-2009 cars

### Removal Procedure

1. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement .
2. Turn the ignition lock cylinder to the accessory position.
3. Insert the 90 degree tip of a pick type tool into the ignition lock cylinder access hole.
4. Push and hold the ignition lock cylinder retaining pin down.
5. Pull the ignition lock cylinder away from the steering column.

### Installation Procedure

1. Install the ignition lock cylinder by performing the following procedure:

1.1. | Turn the ignition lock cylinder to the accessory position.

1.2. | Push the ignition lock cylinder in until the retaining pin locks it in place.

2. Install the steering column trim covers. Refer to Steering Column Trim Covers Replacement .