For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Stabilizer Shaft Bushing Clamp Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 50N·m (37 lb ft).
2 | Stabilizer Shaft Bushing Clamp
3 | Stabilizer Shaft Bushing Tip When installing the bushing, ensure that the slit in the bushing is facing the front of the vehicle.