For 1990-2009 cars
Master Electrical Component List
Automatic Transmission Controls Schematics
OBD II Symbol Description Notice

### Circuit Description

The torque converter clutch (TCC) solenoid valve is a normally-open exhaust valve that is used with the torque converter clutch pulse width modulation (TCC PWM) solenoid valve in order to control fluid acting on the converter clutch apply valve. The TCC solenoid valve attaches to the transmission case assembly extending into the pump cover. When grounded, energized, by the powertrain control module (PCM), the TCC solenoid valve stops converter signal oil from exhausting. This causes converter signal oil pressure to increase and move the converter clutch apply valve against spring force and into the apply position. In this position, release fluid is open to an exhaust port and converter feed fluid fills the apply fluid circuit. The converter feed fluid applies the TCC. When the PCM no longer provides a ground path, the TCC solenoid valve de-energizes and apply fluid exhausts, releasing the TCC.

When the PCM detects low TCC slip when the TCC is commanded OFF, then DTC P0742 sets. DTC P0742 is a type B DTC.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC P0742 Torque Converter Clutch (TCC) System - Stuck On

### Conditions for Running the DTC

• | No vehicle speed sensor (VSS) DTCs P0502 or P0503.

• | No transmission fluid pressure (TFP) manual valve position switch DTC P1810, P1815 or P1816.

• | No TCC PWM solenoid valve DTC P2763 or P2764.

• | No TCC Stuck Off DTC P0741.

• | The throttle position (TP) angle is 10-90 percent.

• | The engine speed is greater than 475 RPM for 6 seconds.

• | The engine is not in fuel cutoff.

• | The transmission fluid temperature (TFT) is between 20-130°C (68-266°F).

• | The engine torque is 70-525 N·m (50-400 lb ft).

• | The engine speed is 750-4,500 RPM.

• | Estimated Gear Ratio is 0.95-1.52.

• | The vehicle speed is 25-140 km/h (15-87 mph).

• | The gear range does not change within 5 seconds.

• | The commanded gear is not 1st.

• | The gear range is D4.

• | The TCC is commanded OFF.

### Conditions for Setting the DTC

DTC P0742 sets if the following condition occurs 3 times.

The TCC slip speed is -20 to +25 RPM for 5 seconds.

### Action Taken When the DTC Sets

• | The PCM illuminates the malfunction indicator lamp (MIL) during the second consecutive trip in which the Conditions for Setting the DTC are met.

• | The PCM commands maximum line pressure.

• | The PCM commands TCC OFF.

• | The PCM freezes shift adapts from being updated.

• | The PCM records the operating conditions when the Conditions for Setting the DTC are met. The PCM stores this information as Freeze Frame and Failure Records.

• | The PCM stores DTC P0742 in PCM history during the second consecutive trip in which the Conditions for Setting the DTC are met.

### Conditions for Clearing the MIL/DTC

• | The PCM turns OFF the MIL during the third consecutive trip in which the diagnostic test runs and passes.

• | A scan tool can clear the MIL/DTC.

• | The PCM clears the DTC from PCM history if the vehicle completes 40 warm-up cycles without an emission-related diagnostic fault occurring.

• | The PCM cancels the DTC default actions when the fault no longer exists and/or the ignition switch is OFF long enough in order to power down the PCM.

### Diagnostic Aids

The TCC fluid hydraulically applies the TCC, possibly causing an engine stall, under the following conditions:

• | The TCC is hydraulically stuck ON

• | The parking brake is applied

• | Any gear range is selected

### Test Description

The number below refers to the step number on the diagnostic table.

1. This step tests the hydraulic state of the TCC. When the PCM commands the TCC solenoid valve OFF, the slip speed should increase.

#### DTC P0742

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.

Important: Before clearing the DTC, use the scan tool in order to record the Freeze Frame and Failure Records. Using the Clear Info. function erases the Freeze Frame and Failure Records from the powertrain control module (PCM).

3. Record the DTC Freeze Frame and Failure Records.
4. Clear the DTC.
5. Drive the vehicle in the D4 drive range in second, third, or fourth gear under steady acceleration, with a TP angle at 20 percent.

While the scan tool TCC Enable status is NO, does the scan tool display a TCC Slip Speed within the specified range?

-20 to +20 RPM

Go to Step 3

Go to Diagnostic Aids

3 | The TCC is hydraulically stuck ON. Inspect for the following:

• | Clogged exhaust orifice in the TCC solenoid valve.

• | Converter clutch apply valve stuck in the apply position.

• | Misaligned or damaged valve body gasket.

• | Restricted release passage.

• | Restricted transmission cooler line.

Did you find and correct the condition?

--

Go to Step 4

--

4 | Perform the following procedure in order to verify the repair:

1. Select DTC.
2. Select Clear Info.
3. Drive the vehicle in D4 with the TCC OFF and the throttle above 17 percent. Ensure that the scan tool TCC Slip Speed is 100-2,000 RPM for 4 seconds.
4. Select Specific DTC.
5. Enter DTC P0742.

Has the test run and passed?

--

Go to Step 5

Go to Step 2

5 | With the scan tool, observe the stored information, capture info, and DTC Info. Does the scan tool display any DTCs that you have not diagnosed? | -- | Go to Diagnostic Trouble Code (DTC) List - Vehicle | System OK