For 1990-2009 cars

### Removal Procedure

1. Remove the seat back recliner handle. Refer to Driver Seat and Passenger Seat Recliner Handle Replacement .
2. Remove the 3 screws retaining the trim panel to the seat.
3. Remove the front seat cushion outer trim panel from the vehicle.

### Installation Procedure

1. Align the front seat cushion outer trim panel to the seat assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the 3 seat cushion outer trim panel mounting screws.

Tighten
Tighten the front seat cushion outer trim panel screws to 1.5 N·m (13 lb in).

3. Install the seat back recliner handle. Refer to Driver Seat and Passenger Seat Recliner Handle Replacement .