For 1990-2009 cars

### Removal Procedure

1. Remove the bumper bracket. Refer to Rear Bumper Bracket Replacement .
2. Remove the hitch bolts from the frame.
3. Remove the hitch from the vehicle.

### Installation Procedure

1. Install the hitch to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the hitch bolts to the frame.

Tighten
Tighten the bolts to 100 N·m (74 lb ft).

3. Install the bumper bracket. Refer to Rear Bumper Bracket Replacement .