For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Moveable Window Schematics Connector End View Reference: Window Systems Connector End Views
1 | Did you review the Power Windows Description and Operation? | Go to Step 2 | Go to Symptoms - Fixed and Moveable Windows
2 | Verify that the power windows express down function is inoperative. Does the power windows express down function operate normally? | Go to Testing for Intermittent Conditions and Poor Connections | Go to Step 3
3 | Inspect for poor connections at the harness connector of the driver window switch. Refer to Testing for Intermittent Conditions and Poor Connections and to Connector Repairs . Did you find and correct the condition? | Go to Step 5 | Go to Step 4
4 | Replace the driver window switch. Refer to Entertainment/Communication Component Views . Did you complete the replacement? | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2