For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws and washers (4) securing the sunshade (1) to the roof.
2. Remove the sunshade assembly.
3. Remove the screw and washer (3) securing the sunshade retainer (2) to the roof.
4. Remove the sunshade retainer.

### Installation Procedure

1. Install the sunshade retainer.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the screw and washer (3) securing the sunshade retainer (2) to the roof.

Tighten
Tighten the sunshade retainer screw to 1.2 N·m (10 lb in).

3. Install the sunshade assembly to the roof with 2 screws and washers.

Tighten
Tighten the sunshade screws to 1.2 N·m (10 lb in).