For 1990-2009 cars

1. Install the parking lock bracket (86).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the parking lock bracket bolt (87) and tighten to 31 N·m (23 lb ft).
3. Inspect the following items:

• | The parking brake pawl (81) for damage or cracks

• | The parking pawl return spring (80) for being broken or missing

4. Inspect the following items:

• | Manual shaft (84) for damage or burrs

• | Parking lock actuator assembly (85) for damage

• | Manual shift detent lever with shaft position switch assembly (88) for damage or cracks

• | Manual valve link (89) for damage

• | Manual shift detent lever pin (92) discard, do not reuse

5. Install the following items:

• | Manual shift detent lever with shaft position switch assembly (88)

• | Parking lock actuator assembly (85)

• | Manual shaft (84) (model dependent)

• | NEW manual shift detent lever pin (92)

• | Manual valve link (89)