For 1990-2009 cars

#### Special Tools

J 9886-01 Door Handle Clip Remover

### Removal Procedure

1. Remove the window regulator handle from the door by inserting tool J 9886-01 between the handle and the white plastic washer to remove the retaining clip, if the vehicle is equipped with manual windows.
2. Remove the retaining screw from the door handle bezel.
3. Remove the 2 retaining screws from the armrest.
4. Disconnect the electrical harness from the power window switch, if equipped.
5. Gently pull the door panel away from the door.
6. Remove any fasteners from the door and reinsert them in the door panel before installing the panel on the door.

### Installation Procedure

1. Install the trim panel to the door, ensuring that all the retaining tabs are fully seated.
2. Connect the electrical harness to the power window switch, if equipped.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the 2 retaining screws in the switch plate. Tighten the rear door switch plate screws to 2 N·m (18 lb in).
4. Install the retaining screw in the door handle bezel. Tighten the rear door handle bezel screws to 2 N·m (18 lb in).
5. Install the window regulator handle from the door and insert the clip between the handle and the white plastic washer, if the vehicle is equipped with manual windows.