For 1990-2009 cars

#### Special Tools

J 24319-B Steering Linkage and Tie Rod Puller

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the outer tie rod retaining nut. Discard the nut.

Caution: Do not attempt to disconnect a steering linkage joint by driving a wedge between the joint and the attached part. Seal damage may result which will cause premature failure of the joint.

4. Disconnect the outer tie rod from the steering knuckle using J 24319-B .
5. Loosen the jam nut and remove the outer tie rod from the inner tie rod. Discard the jam nut.
6. Clean the tapered surface of the steering knuckle.

### Installation Procedure

1. Lubricate the inner tie rod threads with a suitable chassis lubricant before installing the outer tie rod.
2. Install the NEW jam nut to the outer tie rod.
3. Install the outer tie rod to the inner tie rod.
4. Install the outer tie rod to the steering knuckle.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the NEW outer tie rod retaining nut.

• | Tighten the outer tie rod retaining nut to 45 N·m (33 lb ft) plus 95 degrees.

• | Tighten the outer tie rod end jam nut to 70 N·m (52 lb ft).

6. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation.
7. Lower the vehicle.
8. Adjust the front toe. Refer to Front Toe Adjustment.