For 1990-2009 cars

#### Special Tools

• | J 23327-1 Forward Clutch Spring Compressor (Bridge)

• | J 34627 Snap Ring Remover and Installer

• | J-42628 Plate

1. Install the J 23327-1 compressor (bridge) and the J-42628 plate .
2. Tighten the J 23327-1 compressor (bridge) .
3. Remove the low and reverse clutch retainer ring (693) using the J 34627 remover and installer .
4. Remove the low and reverse clutch spring assembly (694).
5. Blow compressed air into the case passage to remove the low and reverse clutch piston (695).

• | (1) LO Feed Passage

• | (2) REV Feed Passage